[bookmark: _Toc42488099]ANNEX IV : Budget breakdown (Model financial offer) 
Nota Bene: All amounts are to be quoted excluding taxes. VAT, if applicable, is to be mentioned separately. Please refer to tender documents, notably the Instructions to tenderers, section 11 Content of tenders. 
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	E

	ITEM NUMBER
	DESCRIPTION 
	UNIT 
	QUANTITY
	SPECIFICATIONS OFFERED (INCL BRAND/MODEL)
	UNIT COSTS WITH DELIVERY DDP[footnoteRef:1] RESEN [1: 	[DDP (D6elivered Duty Paid)][DAP (Delivered At Place)]  — Incoterms 2020 International Chamber of Commerce http://www.iccwbo.org/incoterms/ ] 

EUR
	TOTAL
EUR

	1 

	Half-cut monocrystalline photovoltaic modules with a power output of 500 Wp 
Dimensions of 1,909 × 1,134 × 30 mm
	piece
	40
	 
	
	

	2  
	Aluminum profiles as a structural framework, including all necessary connecting elements, with a length of 50 cm or similar
	piece
	98
	
	
	

	3
	Aluminum end clamps for securing the modules
	piece
	36
	
	
	

	4
	Aluminum mid clamps for securing the modules
	[bookmark: _GoBack]piece
	62
	
	
	

	5
	Three-phase inverter with a nominal power output of 17.50 kW, equipped with integrated DC and AC surge protection devices and an integrated plant monitoring system. 
Reference type: Fronius Symo Advanced 17.5-3-M or equivalent
Warranty 5 years
	piece
	1
	
	
	

	6
	AC cabinet with 
•	dimensions of 400 × 500 × 200 mm,  
•	minimum mechanical protection rating of  IP65, 
•	impact resistance IK08, 
•	Protection Class II, 
•	halogen-free construction, 
•	UV- and weather-resistant eclosure, 
•	Suitable for a rated voltage of up to 400 V and an operating temperature range of -25 to +60 °C, with cable glands at the bottom. 
The cabinet shall be wall-mounted and equipped with the following: Two three-pole circuit breakers, rated at 32 A with C characteristic , one three-pole circuit breaker rated at 63 A with C characteristic, Neutral (N) busbar, Protective earth (PE) busbar, Cable glands at the bottom
All components shall be suitable for the intended AC photovoltaic installation and shall comply with the applicable IEC/EN standards and relevant safety requirements
	piece
	1
	
	
	

	7
	Power cable: PP 00-Y 5 × 6 mm², 0.6/1 kV
	m
	6
	
	
	

	8
	Power cable: PP 00 4 × 16 mm², 0.6/1 kV
	m
	6
	
	
	

	9
	Single-core cable: P/F-Y 1 × 16 mm²
	m
	36
	
	
	

	10
	Solar cable: PV1-F 1 × 6 mm², 1.8 kV
	m
	300
	
	
	

	11
	MC4 (+) connectors and pins
	piece
	5
	
	
	

	12
	MC4 (- ) connectors and pins
	piece
	5
	
	
	

	13
	Perforated cable tray with covers, dimensions 50 × 60 mm ,
	lump sum
	1
	
	
	

	14
	Silicone, corrugated, self-extinguishing conduit, Ø 20–32 mm
	m
	50
	
	
	

	15
	Three-pole circuit breaker, rated at 63 A, with C characteristic
	piece 
	1
	
	
	

	16
	Miscellaneous installation materials
	lump sum
	1
	
	
	

	17
	Complete technical documentation according to national law and legislation  
	piece  
	1
	
	
	

	18
	Installation and login to mobile application to record PV station parameters and training of two responsible employees  
	lump sum
	1
	
	
	

	19
	Supply, transport and installation of a dual-outlet AC charging station for electric vehicles
	piece
	2
	
	
	

	20
	Additional equipment, occurred due to unexpected situation, from those planned in tech. document (max 10%)
	lump sum
	1
	
	
	

	21
	Information plaque with dimensions of 300 × 400 mm, manufactured from durable and weather-resistant material, such as metal with a protective coating, in accordance with the visibility and communication requirements of the Interreg VI-A Greece–North Macedonia 2021–2027 Programme.
	piece
	2
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