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Columns 1-2 should be completed by the contracting authority
Columns 3-4 should be completed by the tenderer
[bookmark: _GoBack]Column 5 is reserved for the evaluation committee 
Annex III - the contractor's technical offer
The tenderers are requested to complete the template on the next pages: 
· Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer), 
· Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)  
· Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation
The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.
The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offered specifications.





LOT 1: Supply of 2 (two) Telescopes
	1.
Item number
	2.
Specifications required
	3.
Specifications offered
	4. 
Notes, remarks, 
ref to documentation
	5.
Evaluation committee’s notes 

	1.
	2 (two) Telescopes
	 
	
	

	
	Objective/aperture: 70–82 mm
	
	
	

	
	Magnification: 20–60x zoom
	 
	
	

	
	Eyepieces: Quality zoom (20–60x) and (12–20 mm)
	
	
	

	
	Coatings: Fully multi-coated (FMC) optics
	
	
	

	
	Close focus: ≤3–4 m for nearby birds/animals
	
	
	

	
	Eye relief: ≥15 mm
	
	
	

	
	Mechanical / mount
	
	
	

	
	Tripod: Sturdy aluminum or light carbon-fiber tripod
	
	
	

	
	Weight 3–6 kg
	
	
	

	
	Weatherproofing: Waterproof and nitrogen- or argon-filled
	
	
	

	
	Controls: Smooth zoom/focus knobs with good tactile feedback.
	
	
	

	
	Accessories: Padded carry case or bag Lens caps, rain/shade hood, cleaning kit Protective eyepiece cover / dust cap
	
	
	

	
	Minimum 2 (two) years warranty
	
	
	




the Incoterm applicable shall be DDP Resen . The equipment must be delivered in Resen. 
* The contractor must provide guideline and short presentation for using equipment to the employees in Municipality of Resen; 






















LOT 2: Supply of 3 (three) Cameras-Photo traps
	1.
Item number
	2.
Specifications required
	3.
Specifications offered
	4. 
Notes, remarks, 
ref to documentation
	5.
Evaluation committee’s notes 

	1.
	3 (three) Cameras-Photo traps
	 
	
	

	
	Image sensor: min 5 megapixel color CMOS
	
	
	

	
	Day/night mode: Yes
	 
	
	

	
	IR range: min 2 0 m
	
	
	

	
	Memory: SD card (8MB - 32GB)
	
	
	

	
	LEDs: min 20 pieces without glow
	
	
	

	
	Lens: min F=1.8; FOV=120°;
	
	
	

	
	Photo size: 8 MP / 14 MP / 36 MP
	
	
	

	
	Photo format: JPEG
	
	
	

	
	Video resolution: min 1080P , 4K 
	
	
	

	
	Video length: 5–180 sec., programmable
	
	
	

	
	Shutter speed: min 0.3 s
	
	
	

	
	Power supply: Batteries
	
	
	

	
	GPRS Email: Yes MMS Phone: Yes
	
	
	

	
	Sending large images: Support sending original images Sending video: Supported sending video
	
	
	

	
	Low battery warning
	
	
	

	
	Interface: USB / SD card / DC port / Micro SIM card
	
	
	

	
	Mounting: Strap; tripod
	
	
	

	
	Operating temperature: -40°C to 60°C
	
	
	

	
	Storage temperature: -40°C to 70°C
	
	
	

	
	Operating humidity: 5% - 90%
	
	
	

	
	Waterproof: IP67
	
	
	

	
	1 set of batteries
	
	
	

	
	Minimum 2 (two) years warranty
	
	
	



the Incoterm applicable shall be DDP Resen . The equipment must be delivered in Resen. 
* The contractor must provide guideline and short presentation for using equipment to the employees in Municipality of Resen; 
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